**Traffic Suitability.**

There is a requirement for eyecare manufacturers to inform eyecare professionals about the suitability of lenses provided for driving.

**Not suitable.**

With eyeglasses, the tint of which does not ensure traffic light recognition in accordance with

DIN EN ISO 14880, the manufacturer must inform the eyecare professional about this

restriction in use.

**Daytime only.**

The manufacturer of eyeglass lenses featuring light reduction of more than 25% (in accordance

with DIN EN ISO 14889) must inform the eyecare professional about such restrictions in use.

In order to do this then there are the following updates.

In the lens technical data, there is a traffic suitability option. There are 3 options.

No restrictions (default)

No suitable for driving

Suitable for daytime only.

In the tint options screen, there is an equivalent screen.

When an order is added, loaded from an edi order file or amended then the lens technical data and the tint option data is checked and the highest traffic restriction is obtained and saved on the order.

In view job this is shown in the top right hand corner as a code 1,2 or 3. If the mouse is hovered over then the text of the restriction is shown. The text can be set is settings / despatch / traffic suitability.

There is a layout tag <TRAFFIC> which can be used on the order and delivery prints.